|  |
| --- |
| **MAKING A CALL** |
| Lift the Handset or press **Speaker** (For the remainder of this guide we will refer to lifting the handset but pressing the **Speaker** key is also valid)* Dial the required internal number
* For external calls, dial **0** first for an outside line
 |

|  |
| --- |
| **HOLD** |
| Ask the caller to please hold:* Press **Hold** - hold key flashes.
* You may replace handset if you wish.

*To retrieve a call:** Lift the handset.
* Press the **Flashing Line Key**
 |

|  |
| --- |
| **TRANSFER** |
| With a call in progress:* Press **Transfer**
* Dial an extension, external number or programmed one-touch key and announce the call when they answer (optional)
* Replace the handset

*Note:* If the called extension is busy or does not answer, press the **Green** **Flashing Key** to return to your caller. If the extension answers and indicates that they do not wish to take the call, ask them to hang up and you will be put directly back to the original caller. |

|  |
| --- |
| **REDIAL** |
| **Last dialed number*** Lift the handset and press **#5** to initiate the call

**Recently dialed numbers*** Without lifting handset press **Redial** (Right Cursor key).
* Press the Cursor button up or down to search for the required number
* Lift the handset to initiate the call
 |

|  |
| --- |
| **CONFERENCE** |
| With a call in progress (internal or external)* Press the **More** soft key and then the **Conf** soft key
* Dial an internal or external number
* When the third party answers, press the

**Add** soft key*Repeat the above 3 steps until all parties are in the conference.* Then press the **Begin** soft key to begin the conference*Note:* Any party may exit the conference by hanging up. As long as at least one of the parties is an extension on the phone system the conference will remain active. |

|  |
| --- |
| **CALL PICK UP** |
| To answer a ringing extension in your group:* Lift the handset and dial **\* #**

To answer a call ringing at a specific extension:* Lift the handset and dial **\* \***

plus the other extensions number |

|  |
| --- |
| **SPEED DIALING** |
| **To dial a system speed dial:*** Lift the handset
* Dial **#2**
* Dial the 3 digit speed dial location (000 ~ 899)

*- Or* - Without lifting the handset, * Press **Directory** (Down Cursor key)
* Press the Cursor button up or down to search for the required number
* Press the lift the handset to initiate the call

**To add a system speed dial:*** Press the Speaker key and dial **753**
* Dial the speed dial location (000 ~ 899)
* Dial telephone number you want to store (up to 24 digits)
* Press **Hold** to store
* If desired, enter name using dial pad
* Press **Hold** to store

*Note:* To move the cursor right press **#** , to move the cursor left press **Clear/Back** |

|  |
| --- |
| **VOICE CALL ANNOUNCE** |
| Allows the caller to make the receiver’s digital phone automatically answer the internal call and go directly to speaker/hands free.* Lift the handset and dial the extension number
* Press **Voice** soft key *or* dial **1** while the other phone is still ringing and speak over the intercom
 |

|  |
| --- |
| **AUTO HANDSFREE ANSWER** |
| Incoming internal calls to the digital extension are automatically answered and put on hands free/speaker.*To Activate:** Press the Speaker key and dial **721**

*To Cancel:** Press the Speaker key and dial **723**
 |

|  |
| --- |
| **PAGING** |
| Allows a user to page all digital handsets.* Lift the handset and dial **\*10**
 |

|  |
| --- |
| **VOICEMAIL** |
| **To access your mailbox and retrieve messages:*** Push the **VM** soft key, or
* Lift the handset and dial **\*8**

**To record a greeting for your mailbox:** Access your mailbox, then using the soft keys below the display select:* **Greet,**
* **Gr1, Gr2 or Gr3,**
* **Rec**
* Speak into the handset after the tone.
* Once you are done recording press **#**

*Use the* **Lstn***soft key to playback the greeting***To forwards calls to your mailbox:**when your extension is busy or after the no answer timer expires* Press the Speaker key and dial **744**
* Dial **1** to set
* Dial the destination number **199**
* Press **Speaker** to store

*To Cancel:** Press the Speaker key and dial **744**

Dial **0**  to cancel. |

|  |
| --- |
| **PROGRAMMING ONE-TOUCH KEYS** |
| To program an extension or an external number into a vacant function key* Press the Speaker key and dial **751**
* Press an available Function key
* Dial the *One-Touch* service code **01**
* Enter either an extension number or external number, including 0 for an outside line
* Press **Hold** to store

*Service Code* **00** *will erase data from function key* |

|  |
| --- |
| **EXTENSION NAME** |
| To edit the displayed extension name of any extension* Press the **Speaker** key and dial **700**
* Enter the number of the extension to change
* Enter the name using the dial pad
* Press **Hold** to store

*Note:* To move the cursor right press **#** , to move the cursor left press **Clear/Back** |

|  |
| --- |
| **LCD** |
| To adjust the display contrast* Press **Menu** (Center Cursor Key)
* Dial **21** and press the **Select** soft key
* Use the cursor button up or down to adjust the display contrast
 |

|  |
| --- |
| **SPEAKER/RECEIVER VOLUME** |
| To adjust the speaker/receiver volume* Press the Cursor key up or down during a phone conversation
 |

|  |
| --- |
| **RINGER VOLUME** |
| To adjust the ringer volume* Press the Cursor key up or down while the phone is ringing
 |

|  |
| --- |
| **KEY PAD TONES** |
| To activate key pad tones* Press the Speaker key and dial **724** to turn On/Off
 |

|  |
| --- |
| **CLOCK** |
| To change the time displayed on all handsets* Lift the handset and dial **728**
* Enter the time in 24hr format (e.g. 9am – 0900)
* Confirmation tone will be heard after entering the digits, then replace the handset
 |

|  |
| --- |
| **BACKGROUND MUSIC** |
| To listen to the background music source through the loud speaker of a digital handset* Press the Speaker key and dial #**725** to turn On/Off
 |

|  |
| --- |
| **24 Button Telephone** |
| **HANDSET CONTROLS** |
| **Call Indicator Lamp**This lamp flashes fast when a call is ringing, or flashes slower when a message has been left.**Alphanumeric Display**The LCD has 3 lines, 24 characters with backlight.**Exit**Exit any screen and return the display to “Time and Date”.**Help Key**Explanations of Programmable Keys can be called up on the LCD by pressing and holding the Help key plus Programmable key**Soft Keys**The Soft Keys show the available features for your current activity. Any feature shown at the bottom of the LCD is available. |
| **Programmable Function Keys**Flexible Line keys or Feature keys are assigned by function code 751 *see previous page***Flash Key**Press key to finish an outside call and hear the dial tone**Transfer Key**Allows the extension user to transfer established calls to another extension**Mute (Microphone) Key**Mute handset or handsfree microphone. LED lights when microphone is muted**DND (Do Not Disturb) Key**Set up a Do Not Disturb if pressed during a call**Clear/Back Key**Press this key to cancel the current action or delete a character**Cursor Key**Access various features with simple operation**Speaker**Controls built-in speaker, which can be used for Hands Free Dialing/Monitoring. LED on key lights when key is active**Hold**Press this key to place an internal or external call on hold |